Skip to main content
`Ctrl`+`K`
scipy.signal.

# lfilter

scipy.signal.lfilter(b, a, x, axis=-1, zi=None)

  Filter data along one-dimension with an IIR or FIR filter.

  Filter a data sequence, x, using a digital filter. This works for many fundamental data types (including Object type). The filter is a direct form II transposed implementation of the standard difference equation (see Notes).

  The function `sosfilt` (and filter design using `output='sos'`) should be preferred over `lfilter` for most filtering tasks, as second-order sections have fewer numerical problems.

  Parameters:
    b array_like

      The numerator coefficient vector in a 1-D sequence.

    a array_like

      The denominator coefficient vector in a 1-D sequence. If `a[0]` is not 1, then both a and b are normalized by `a[0]`.

    x array_like

      An N-dimensional input array.

    axis int, optional

      The axis of the input data array along which to apply the linear filter. The filter is applied to each subarray along this axis. Default is -1.

    zi array_like, optional

      Initial conditions for the filter delays. It is a vector (or array of vectors for an N-dimensional input) of length `max(len(a), len(b)) - 1`. If zi is None or is not given then initial rest is assumed. See `lfiltic` for more information.

  Returns:
    y array

      The output of the digital filter.

    zf array, optional

      If zi is None, this is not returned, otherwise, zf holds the final filter delay values.

  See also

  `lfiltic`

    Construct initial conditions for `lfilter`.

  `lfilter_zi`

    Compute initial state (steady state of step response) for `lfilter`.

  `filtfilt`

    A forward-backward filter, to obtain a filter with zero phase.

  `savgol_filter`

    A Savitzky-Golay filter.

  `sosfilt`

    Filter data using cascaded second-order sections.

  `sosfiltfilt`

    A forward-backward filter using second-order sections.

  Notes

  The filter function is implemented as a direct II transposed structure. This means that the filter implements:

      a[0]*y[n] = b[0]*x[n] + b[1]*x[n-1] + ... + b[M]*x[n-M]
                            - a[1]*y[n-1] - ... - a[N]*y[n-N]

  where M is the degree of the numerator, N is the degree of the denominator, and n is the sample number. It is implemented using the following difference equations (assuming M = N):

      a[0]*y[n] = b[0] * x[n]               + d[0][n-1]
        d[0][n] = b[1] * x[n] - a[1] * y[n] + d[1][n-1]
        d[1][n] = b[2] * x[n] - a[2] * y[n] + d[2][n-1]
      ...
      d[N-2][n] = b[N-1]*x[n] - a[N-1]*y[n] + d[N-1][n-1]
      d[N-1][n] = b[N] * x[n] - a[N] * y[n]

  where d are the state variables.

  The rational transfer function describing this filter in the z-transform domain is:

                          -1              -M
              b[0] + b[1]z  + ... + b[M] z
      Y(z) = -------------------------------- X(z)
                          -1              -N
              a[0] + a[1]z  + ... + a[N] z

  Examples

  Generate a noisy signal to be filtered:

      >>> import numpy as np
      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt
      >>> rng = np.random.default_rng()
      >>> t = np.linspace(-1, 1, 201)
      >>> x = (np.sin(2*np.pi*0.75*t*(1-t) + 2.1) +
      ...      0.1*np.sin(2*np.pi*1.25*t + 1) +
      ...      0.18*np.cos(2*np.pi*3.85*t))
      >>> xn = x + rng.standard_normal(len(t)) * 0.08

  Create an order 3 lowpass butterworth filter:

      >>> b, a = signal.butter(3, 0.05)

  Apply the filter to xn. Use lfilter_zi to choose the initial condition of the filter:

      >>> zi = signal.lfilter_zi(b, a)
      >>> z, _ = signal.lfilter(b, a, xn, zi=zi*xn[0])

  Apply the filter again, to have a result filtered at an order the same as filtfilt:

      >>> z2, _ = signal.lfilter(b, a, z, zi=zi*z[0])

  Use filtfilt to apply the filter:

      >>> y = signal.filtfilt(b, a, xn)

  Plot the original signal and the various filtered versions:

      >>> plt.figure
      >>> plt.plot(t, xn, 'b', alpha=0.75)
      >>> plt.plot(t, z, 'r--', t, z2, 'r', t, y, 'k')
      >>> plt.legend(('noisy signal', 'lfilter, once', 'lfilter, twice',
      ...             'filtfilt'), loc='best')
      >>> plt.grid(True)
      >>> plt.show()