Skip to main content
`Ctrl`+`K`
scipy.signal.

# firwin_2d

scipy.signal.firwin_2d(hsize, window, *, fc=None, fs=2, circular=False, pass_zero=True, scale=True)

  2D FIR filter design using the window method.

  This function computes the coefficients of a 2D finite impulse response filter. The filter is separable with linear phase; it will be designed as a product of two 1D filters with dimensions defined by hsize. Additionally, it can create approximately circularly symmetric 2-D windows.

  Parameters:
    hsizetuple or list of length 2

      Lengths of the filter in each dimension. hsize[0] specifies the number of coefficients in the row direction and hsize[1] specifies the number of coefficients in the column direction.

    windowtuple or list of length 2 or string

      Desired window to use for each 1D filter or a single window type for creating circularly symmetric 2-D windows. Each element should be a string or tuple of string and parameter values. See `get_window` for a list of windows and required parameters.

    fcfloat or 1-D array_like, optional

      Cutoff frequency of the filter in the same units as fs. This defines the frequency at which the filter’s gain drops to approximately -6 dB (half power) in a low-pass or high-pass filter. For multi-band filters, fc can be an array of cutoff frequencies (i.e., band edges) in the range [0, fs/2], with each band specified in pairs. Required if circular is False.

    fsfloat, optional

      The sampling frequency of the signal. Default is 2.

    circularbool, optional

      Whether to create a circularly symmetric 2-D window. Default is `False`.

    pass_zero{True, False, ‘bandpass’, ‘lowpass’, ‘highpass’, ‘bandstop’}, optional

      This parameter is directly passed to `firwin` for each scalar frequency axis. Hence, if `True`, the DC gain, i.e., the gain at frequency (0, 0), is 1. If `False`, the DC gain is 0 at frequency (0, 0) if circular is `True`. If circular is `False` the frequencies (0, f1) and (f0, 0) will have gain 0. It can also be a string argument for the desired filter type (equivalent to `btype` in IIR design functions).

    scalebool, optional

      This parameter is directly passed to `firwin` for each scalar frequency axis. Set to `True` to scale the coefficients so that the frequency response is exactly unity at a certain frequency on one frequency axis. That frequency is either:

      - 0 (DC) if the first passband starts at 0 (i.e. pass_zero is `True`)

      - fs/2 (the Nyquist frequency) if the first passband ends at fs/2 (i.e., the filter is a single band highpass filter); center of first passband otherwise

  Returns:
    filter_2d(hsize[0], hsize[1]) ndarray

      Coefficients of 2D FIR filter.

  Raises:
    ValueError

      - If hsize and window are not 2-element tuples or lists.

      - If cutoff is None when circular is True.

      - If cutoff is outside the range [0, fs/2] and circular is `False`.

      - If any of the elements in window are not recognized.

    RuntimeError

      If `firwin` fails to converge when designing the filter.

  See also

  `firwin`

    FIR filter design using the window method for 1d arrays.

  `get_window`

    Return a window of a given length and type.

  Examples

  Generate a 5x5 low-pass filter with cutoff frequency 0.1:

      >>> import numpy as np
      >>> from scipy.signal import get_window
      >>> from scipy.signal import firwin_2d
      >>> hsize = (5, 5)
      >>> window = (("kaiser", 5.0), ("kaiser", 5.0))
      >>> fc = 0.1
      >>> filter_2d = firwin_2d(hsize, window, fc=fc)
      >>> filter_2d
      array([[0.00025366, 0.00401662, 0.00738617, 0.00401662, 0.00025366],
             [0.00401662, 0.06360159, 0.11695714, 0.06360159, 0.00401662],
             [0.00738617, 0.11695714, 0.21507283, 0.11695714, 0.00738617],
             [0.00401662, 0.06360159, 0.11695714, 0.06360159, 0.00401662],
             [0.00025366, 0.00401662, 0.00738617, 0.00401662, 0.00025366]])

  Generate a circularly symmetric 5x5 low-pass filter with Hamming window:

      >>> filter_2d = firwin_2d((5, 5), 'hamming', fc=fc, circular=True)
      >>> filter_2d
      array([[-0.00020354, -0.00020354, -0.00020354, -0.00020354, -0.00020354],
             [-0.00020354,  0.01506844,  0.09907658,  0.01506844, -0.00020354],
             [-0.00020354,  0.09907658, -0.00020354,  0.09907658, -0.00020354],
             [-0.00020354,  0.01506844,  0.09907658,  0.01506844, -0.00020354],
             [-0.00020354, -0.00020354, -0.00020354, -0.00020354, -0.00020354]])

  Generate Plots comparing the product of two 1d filters with a circular symmetric filter:

      >>> import matplotlib.pyplot as plt
      >>> hsize, fc = (50, 50), 0.05
      >>> window = (("kaiser", 5.0), ("kaiser", 5.0))
      >>> filter0_2d = firwin_2d(hsize, window, fc=fc)
      >>> filter1_2d = firwin_2d((50, 50), 'hamming', fc=fc, circular=True)
      ...
      >>> fg, (ax0, ax1) = plt.subplots(1, 2, tight_layout=True, figsize=(6.5, 3.5))
      >>> ax0.set_title("Product of 2 Windows")
      >>> im0 = ax0.imshow(filter0_2d, cmap='viridis', origin='lower', aspect='equal')
      >>> fg.colorbar(im0, ax=ax0, shrink=0.7)
      >>> ax1.set_title("Circular Window")
      >>> im1 = ax1.imshow(filter1_2d, cmap='plasma', origin='lower', aspect='equal')
      >>> fg.colorbar(im1, ax=ax1, shrink=0.7)
      >>> plt.show()