Skip to main content
`Ctrl`+`K`
scipy.signal.windows.

# boxcar

scipy.signal.windows.boxcar(M, sym=True, *, xp=None, device=None)

  Return a boxcar or rectangular window.

  Also known as a rectangular window or Dirichlet window, this is equivalent to no window at all.

  Parameters:
    Mint

      Number of points in the output window. If zero, an empty array is returned. An exception is thrown when it is negative.

    symbool, optional

      Whether the window is symmetric. (Has no effect for boxcar.)

    xparray_namespace, optional

      Optional array namespace. Should be compatible with the array API standard, or supported by array-api-compat. Default: `numpy`

    device: any

      optional device specification for output. Should match one of the supported device specification in `xp`.

  Returns:
    wndarray

      The window, with the maximum value normalized to 1.

  Examples

  Plot the window and its frequency response:

      >>> import numpy as np
      >>> from scipy import signal
      >>> from scipy.fft import fft, fftshift
      >>> import matplotlib.pyplot as plt

      >>> window = signal.windows.boxcar(51)
      >>> plt.plot(window)
      >>> plt.title("Boxcar window")
      >>> plt.ylabel("Amplitude")
      >>> plt.xlabel("Sample")

      >>> plt.figure()
      >>> A = fft(window, 2048) / (len(window)/2.0)
      >>> freq = np.linspace(-0.5, 0.5, len(A))
      >>> response = 20 * np.log10(np.abs(fftshift(A / abs(A).max())))
      >>> plt.plot(freq, response)
      >>> plt.axis([-0.5, 0.5, -120, 0])
      >>> plt.title("Frequency response of the boxcar window")
      >>> plt.ylabel("Normalized magnitude [dB]")
      >>> plt.xlabel("Normalized frequency [cycles per sample]")