Skip to main content
`Ctrl`+`K`
scipy.signal.

# resample

scipy.signal.resample(x, num, t=None, axis=0, window=None, domain='time')

  Resample x to num samples using the Fourier method along the given axis.

  The resampling is performed by shortening or zero-padding the FFT of x. This has the advantages of providing an ideal antialiasing filter and allowing arbitrary up- or down-sampling ratios. The main drawback is the requirement of assuming x to be a periodic signal.

  Parameters:
    xarray_like

      The input signal made up of equidistant samples. If x is a multidimensional array, the parameter axis specifies the time/frequency axis. It is assumed here that `n_x = x.shape[axis]` specifies the number of samples and `T` the sampling interval.

    numint

      The number of samples of the resampled output signal. It may be larger or smaller than `n_x`.

    tarray_like, optional

      If t is not `None`, then the timestamps of the resampled signal are also returned. t must contain at least the first two timestamps of the input signal x (all others are ignored). The timestamps of the output signal are determined by `t[0] + T * n_x / num * np.arange(num)` with `T = t[1] - t[0]`. Default is `None`.

    axisint, optional

      The time/frequency axis of x along which the resampling take place. The Default is 0.

    windowarray_like, callable, string, float, or tuple, optional

      If not `None`, it specifies a filter in the Fourier domain, which is applied before resampling. I.e., the FFT `X` of x is calculated by `X = W * fft(x, axis=axis)`. `W` may be interpreted as a spectral windowing function `W(f_X)` which consumes the frequencies `f_X = fftfreq(n_x, T)`.

      If window is a 1d array of length `n_x` then `W=window`. If window is a callable then `W = window(f_X)`. Otherwise, window is passed to `get_window`, i.e., `W = fftshift(signal.get_window(window, n_x))`. Default is `None`.

    domain‘time’ | ‘freq’, optional

      If set to `'time'` (default) then an FFT is applied to x, otherwise (`'freq'`) it is asssmued that an FFT was already applied, i.e., `x = fft(x_t, axis=axis)` with `x_t` being the input signal in the time domain.

  Returns:
    x_rndarray

      The resampled signal made up of num samples and sampling interval `T * n_x / num`.

    t_rndarray, optional

      The num equidistant timestamps of x_r. This is only returned if paramater t is not `None`.

  See also

  `decimate`

    Downsample a (periodic/non-periodic) signal after applying an FIR or IIR filter.

  `resample_poly`

    Resample a (periodic/non-periodic) signal using polyphase filtering and an FIR filter.

  Notes

  This function uses the more efficient one-sided FFT, i.e. `rfft` / `irfft`, if x is real-valued and in the time domain. Else, the two-sided FFT, i.e., `fft` / `ifft`, is used (all FFT functions are taken from the `scipy.fft` module).

  If a window is applied to a real-valued x, the one-sided spectral windowing function is determined by taking the average of the negative and the positive frequency component. This ensures that real-valued signals and complex signals with zero imaginary part are treated identically. I.e., passing x or passing `x.astype(np.complex128)` produce the same numeric result.

  If the number of input or output samples are prime or have few prime factors, this function may be slow due to utilizing FFTs. Consult `prev_fast_len` and `next_fast_len` for determining efficient signals lengths. Alternatively, utilizing `resample_poly` to calculate an intermediate signal (as illustrated in the example below) can result in significant speed increases.

  `resample` is intended to be used for periodic signals with equidistant sampling intervals. For non-periodic signals, `resample_poly` may be a better choice. Consult the `scipy.interpolate` module for methods of resampling signals with non-constant sampling intervals.

  Examples

  The following example depicts a signal being up-sampled from 20 samples to 100 samples. The ringing at the beginning of the up-sampled signal is due to interpreting the signal being periodic. The red square in the plot illustrates that periodictiy by showing the first sample of the next cycle of the signal.

      >>> import numpy as np
      >>> import matplotlib.pyplot as plt
      >>> from scipy.signal import resample
      ...
      >>> n0, n1 = 20, 100  # number of samples
      >>> t0 = np.linspace(0, 10, n0, endpoint=False)  # input time stamps
      >>> x0 = np.cos(-t0**2/6)  # input signal
      ...
      >>> x1 = resample(x0, n1)  # resampled signal
      >>> t1 = np.linspace(0, 10, n1, endpoint=False)  # timestamps of x1
      ...
      >>> fig0, ax0 = plt.subplots(1, 1, tight_layout=True)
      >>> ax0.set_title(f"Resampling $x(t)$ from {n0} samples to {n1} samples")
      >>> ax0.set(xlabel="Time $t$", ylabel="Amplitude $x(t)$")
      >>> ax0.plot(t1, x1, '.-', alpha=.5, label=f"Resampled")
      >>> ax0.plot(t0, x0, 'o-', alpha=.5, label="Original")
      >>> ax0.plot(10, x0[0], 'rs', alpha=.5, label="Next Cycle")
      >>> ax0.legend(loc='best')
      >>> ax0.grid(True)
      >>> plt.show()

  The following example compares this function with a naive `rfft` / `irfft` combination: An input signal with a sampling interval of one second is upsampled by a factor of eight. The first figure depicts an odd number of input samples whereas the second figure an even number. The upper subplots show the signals over time: The input samples are marked by large green dots, the upsampled signals by a continuous and a dashed line. The lower subplots show the magnitude spectrum: The FFT values of the input are depicted by large green dots, which lie in the frequency interval [-0.5, 0.5] Hz, whereas the frequency interval of the upsampled signal is [-4, 4] Hz. The continuous green line depicts the upsampled spectrum without antialiasing filter, which is a periodic continuation of the input spectrum. The blue x’s and orange dots depict the FFT values of the signal created by the naive approach as well as this function’s result.

      >>> import matplotlib.pyplot as plt
      >>> import numpy as np
      >>> from scipy.fft import fftshift, fftfreq, fft, rfft, irfft
      >>> from scipy.signal import resample, resample_poly
      ...
      >>> fac, T0, T1 = 8, 1, 1/8  # upsampling factor and sampling intervals
      >>> for n0 in (15, 16):  # number of samples of input signal
      ...     n1 = fac * n0  # number of samples of upsampled signal
      ...     t0, t1 = T0 * np.arange(n0), T1 * np.arange(n1)  # time stamps
      ...     x0 = np.zeros(n0)  # input signal has two non-zero sample values
      ...     x0[n0//2], x0[n0//2+1] = n0 // 2, -(n0 // 2)
      ...
      ...     x1n = irfft(rfft(x0), n=n1) * n1 / n0  # naive resampling
      ...     x1r = resample(x0, n1)  # resample signal
      ...
      ...     # Determine magnitude spectrum:
      ...     x0_up = np.zeros_like(x1r)  # upsampling without antialiasing filter
      ...     x0_up[::n1 // n0] = x0
      ...     X0, X0_up = (fftshift(fft(x_)) / n0 for x_ in (x0, x0_up))
      ...     XX1 = (fftshift(fft(x_)) / n1 for x_ in (x1n, x1r))
      ...     f0, f1 = fftshift(fftfreq(n0, T0)), fftshift(fftfreq(n1, T1))  # frequencies
      ...     df = f0[1] - f0[0]  # frequency resolution
      ...
      ...     fig, (ax0, ax1) = plt.subplots(2, 1, layout='constrained', figsize=(5, 4))
      ...     ax0.set_title(rf"Upsampling ${fac}\times$ from {n0} to {n1} samples")
      ...     ax0.set(xlabel="Time $t$ in seconds", ylabel="Amplitude $x(t)$",
      ...             xlim=(0, n1*T1))
      ...     ax0.step(t0, x0, 'C2o-', where='post', alpha=.3, linewidth=2,
      ...              label="$x_0(t)$ / $X_0(f)$")
      ...     for x_, l_ in zip((x1n, x1r), ('C0--', 'C1-')):
      ...         ax0.plot(t1, x_, l_, alpha=.5, label=None)
      ...     ax0.grid()
      ...     ax1.set(xlabel=rf"Frequency $f$ in hertz ($\Delta f = {df*1e3:.1f}\,$mHz)",
      ...             ylabel="Magnitude $|X(f)|$", xlim=(-0.7, 0.7))
      ...     ax1.axvspan(0.5/T0, f1[-1], color='gray', alpha=.2)
      ...     ax1.axvspan(f1[0], -0.5/T0, color='gray', alpha=.2)
      ...     ax1.plot(f1, abs(X0_up), 'C2-', f0, abs(X0),  'C2o', alpha=.3, linewidth=2)
      ...     for X_, n_, l_ in zip(XX1, ("naive", "resample"), ('C0x--', 'C1.-')):
      ...         ax1.plot(f1, abs(X_), l_, alpha=.5, label=n_)
      ...     ax1.grid()
      ...     fig.legend(loc='outside lower center', ncols=4)
      >>> plt.show()

  The first figure shows that upsampling an odd number of samples produces identical results. The second figure illustrates that the signal produced with the naive approach (dashed blue line) from an even number of samples does not touch all original samples. This deviation is due to `resample` correctly treating unpaired frequency bins. I.e., the input x1 has a bin pair ±0.5 Hz, whereas the output has only one unpaired bin at -0.5 Hz, which demands rescaling of that bin pair. Generally, special treatment is required if `n_x != num` and `min(n_x, num)` is even. If the bin values at ±m are zero, obviously, no special treatment is needed. Consult the source code of `resample` for details.

  The final example shows how to utilize `resample_poly` to speed up the down-sampling: The input signal a non-zero value at \(t=0\) and is downsampled from 19937 to 128 samples. Since 19937 is prime, the FFT is expected to be slow. To speed matters up, `resample_poly` is used to downsample first by a factor of `n0 // n1 = 155` and then pass the result to `resample`. Two parameterization of `resample_poly` are used: Passing `padtype='wrap'` treats the input as being periodic wheras the default parametrization performs zero-padding. The upper subplot shows the resulting signals over time whereas the lower subplot depicts the resulting one-sided magnitude spectra.

      >>> import matplotlib.pyplot as plt
      >>> import numpy as np
      >>> from scipy.fft import rfftfreq, rfft
      >>> from scipy.signal import resample, resample_poly
      ...
      >>> n0 = 19937 # number of input samples - prime
      >>> n1 = 128  # number of output samples - fast FFT length
      >>> T0, T1 = 1/n0, 1/n1  # sampling intervals
      >>> t0, t1 = np.arange(n0)*T0, np.arange(n1)*T1  # time stamps
      ...
      >>> x0 = np.zeros(n0)  # Input has one non-zero sample
      >>> x0[0] = n0
      >>>
      >>> x1r = resample(x0, n1)  # slow due to n0 being prime
      >>> # This is faster:
      >>> x1p = resample(resample_poly(x0, 1, n0 // n1, padtype='wrap'), n1)  # periodic
      >>> x2p = resample(resample_poly(x0, 1, n0 // n1), n1)  # with zero-padding
      ...
      >>> X0 = rfft(x0) / n0
      >>> X1r, X1p, X2p = rfft(x1r) / n1, rfft(x1p) / n1, rfft(x2p) / n1
      >>> f0, f1 = rfftfreq(n0, T0), rfftfreq(n1, T1)
      ...
      >>> fig, (ax0, ax1) = plt.subplots(2, 1, layout='constrained', figsize=(5, 4))
      >>> ax0.set_title(f"Dowsampled Impulse response (from {n0} to {n1} samples)")
      >>> ax0.set(xlabel="Time $t$ in seconds", ylabel="Amplitude $x(t)$", xlim=(-T1, 1))
      >>> for x_ in (x1r, x1p, x2p):
      ...     ax0.plot(t1, x_, alpha=.5)
      >>> ax0.grid()
      >>> ax1.set(xlabel=rf"Frequency $f$ in hertz ($\Delta f = {f1[1]}\,$Hz)",
      ...         ylabel="Magnitude $|X(f)|$", xlim=(0, 0.55/T1))
      >>> ax1.axvspan(0.5/T1, f0[-1], color='gray', alpha=.2)
      >>> ax1.plot(f1, abs(X1r), 'C0.-', alpha=.5, label="resample")
      >>> ax1.plot(f1, abs(X1p), 'C1.-', alpha=.5, label="resample_poly(padtype='wrap')")
      >>> ax1.plot(f1, abs(X2p), 'C2x-', alpha=.5, label="resample_poly")
      >>> ax1.grid()
      >>> fig.legend(loc='outside lower center', ncols=2)
      >>> plt.show()

  The plots show that the results of the “pure” `resample` and the usage of the default parameters of `resample_poly` agree well. The periodic padding of `resample_poly` (`padtype='wrap'`) on the other hand produces significant deviations. This is caused by the disconiuity at the beginning of the signal, for which the default filter of `resample_poly` is not suited well. This example illustrates that for some use cases, adpating the `resample_poly` parameters may be beneficial. `resample` has a big advantage in this regard: It uses the ideal antialiasing filter with the maximum bandwidth by default.

  Note that the doubled spectral magnitude at the Nyqist frequency of 64 Hz is due the even number of `n1=128` output samples, which requires a special treatment as discussed in the previous example.