Skip to main content
`Ctrl`+`K`
scipy.signal.

# dlsim

scipy.signal.dlsim(system, u, t=None, x0=None)

  Simulate output of a discrete-time linear system.

  Parameters:
    systemdlti | tuple

      An instance of the LTI class `dlti` or a tuple describing the system. The number of elements in the tuple determine the interpretation. I.e.:

      - `system`: Instance of LTI class `dlti`. Note that derived instances, such as instances of `TransferFunction`, `ZerosPolesGain`, or `StateSpace`, are allowed as well.

      - `(num, den, dt)`: Rational polynomial as described in `TransferFunction`. The coefficients of the polynomials should be specified in descending exponent order, e.g., z² + 3z + 5 would be represented as `[1, 3, 5]`.

      - `(zeros, poles, gain, dt)`: Zeros, poles, gain form as described in `ZerosPolesGain`.

      - `(A, B, C, D, dt)`: State-space form as described in `StateSpace`.

    uarray_like

      An input array describing the input at each time t (interpolation is assumed between given times). If there are multiple inputs, then each column of the rank-2 array represents an input.

    tarray_like, optional

      The time steps at which the input is defined. If t is given, it must be the same length as u, and the final value in t determines the number of steps returned in the output.

    x0array_like, optional

      The initial conditions on the state vector (zero by default).

  Returns:
    toutndarray

      Time values for the output, as a 1-D array.

    youtndarray

      System response, as a 1-D array.

    xoutndarray, optional

      Time-evolution of the state-vector. Only generated if the input is a `StateSpace` system.

  See also

  `lsim`, `dstep`, `dimpulse`, `cont2discrete`

  Examples

  A simple integrator transfer function with a discrete time step of 1.0 could be implemented as:

      >>> import numpy as np
      >>> from scipy import signal
      >>> tf = ([1.0,], [1.0, -1.0], 1.0)
      >>> t_in = [0.0, 1.0, 2.0, 3.0]
      >>> u = np.asarray([0.0, 0.0, 1.0, 1.0])
      >>> t_out, y = signal.dlsim(tf, u, t=t_in)
      >>> y.T
      array([[ 0.,  0.,  0.,  1.]])