Skip to main content
`Ctrl`+`K`
scipy.signal.

# bode

scipy.signal.bode(system, w=None, n=100)

  Calculate Bode magnitude and phase data of a continuous-time system.

  Parameters:
    systeman instance of the LTI class or a tuple describing the system.

      The following gives the number of elements in the tuple and the interpretation:

      > - 1 (instance of `lti`)

      > - 2 (num, den)

      > - 3 (zeros, poles, gain)

      > - 4 (A, B, C, D)

    warray_like, optional

      Array of frequencies (in rad/s). Magnitude and phase data is calculated for every value in this array. If not given a reasonable set will be calculated.

    nint, optional

      Number of frequency points to compute if w is not given. The n frequencies are logarithmically spaced in an interval chosen to include the influence of the poles and zeros of the system.

  Returns:
    w1D ndarray

      Frequency array [rad/s]

    mag1D ndarray

      Magnitude array [dB]

    phase1D ndarray

      Phase array [deg]

  Notes

  If (num, den) is passed in for `system`, coefficients for both the numerator and denominator should be specified in descending exponent order (e.g. `s^2 + 3s + 5` would be represented as `[1, 3, 5]`).

  Added in version 0.11.0.

  Examples

      >>> from scipy import signal
      >>> import matplotlib.pyplot as plt

      >>> sys = signal.TransferFunction([1], [1, 1])
      >>> w, mag, phase = signal.bode(sys)

      >>> plt.figure()
      >>> plt.semilogx(w, mag)    # Bode magnitude plot
      >>> plt.figure()
      >>> plt.semilogx(w, phase)  # Bode phase plot
      >>> plt.show()